|  |  |  |  |
| --- | --- | --- | --- |
| **HONGER COMBINED DECOILER STRAIGHTENER** |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| **1. CL for small inner diameter coil** |  |  |
|  |  |  |  |  |  |
| **Model** | **CL-150** | **CL-200** | **CL-300** | **CL-400** |  |
| Coil Width (mm) | 100 | 200 | 300 | 400 |  |
| Coil Thickness (mm) | 0.4-2.2 |  |  |  |  |
| Coil I.D. (mm) | 50-530 |  |  |  |  |
| Coil O.D. (mm) | 1000 |  |  |  |  |
| Loading Capacity (kgs) | 300 | 400 | 450 | 500 |  |
| Expansion | Manual |  |  |  |  |
| Straightener Roller | Ø52mm\*7pcs |  |  |  |  |
| Straightener Motor (HP) | 1 | 1 | 2 | 3 |  |
| Roller Pressing  | 4 points |  |  |  |  |
| Roller Adjustment | Spring Adjusting |  |  |  |
| Inverter | Without  |  |  |  |  |
| Feeding Speed (m/min) | 16 |  |  |  |  |
| Uncoiler Motor | Non-motorized |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| **2. GO for material thickness 0.4-2.2mm** |  |  |  |
|  |  |  |  |  |  |
| **Model** | **GO-200** | **GO-300** | **G0-400** | **G0-500** | **GO-600** |
| Coil Width (mm) | 200 | 300 | 400 | 500 | 600 |
| Coil Thickness (mm) | 0.4-2.2 |  |  |  |  |
| Coil I.D. (mm) | 450-530 |  |  |  |  |
| Coil O.D. (mm) | 1200 |  |  |  |  |
| Loading Capacity (kgs) | 800 | 1000 | 1500 | 2000 | 2500 |
| Expansion | Manual |  |  |  |  |
| Straightener Roller | Ø52mm\*7pcs |  |  |  |
| Straightener Motor (HP) | 1 | 2 | 2 | 3 | 3 |
| Roller Pressing  | 4 points |  |  |  |  |
| Roller Adjustment | Spring Adjusting |  |  |  |
| Inverter | Without  |  |  |  |  |
| Feeding Speed (m/min) | 16 |  |  |  |  |
| Uncoiler Motor | Non-motorized |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| **3. GL high precison for material thickness 0.3-3.5mm** |  |  |  |
|  |  |  |  |  |  |
| **Model** | **GL-200** | **GL-300** | **GL-400** | **GL-500** | **GL-600** |
| Coil Width (mm) | 200 | 300 | 400 | 500 | 600 |
| Coil Thickness (mm) | 0.3-3.5 |  |  |  |  |
| Coil I.D. (mm) | 460-520 |  |  |  |  |
| Coil O.D. (mm) | 1200 |  |  |  |  |
| Loading Capacity (kgs) | 600 | 1000 | 1500 | 2000 | 2000 |
| Expansion | Manual |  |  |  |  |
| Straightener Roller | Ø48mm\*7pcs |  |  |  |
| Straightener Motor (HP) | 1 | 2 | 2 | 3 | 3 |
| Roller Pressing  | Pneumatic Rod |  |  |  |
| Roller Adjustment | Eccentric turbine worm adjusting |  |  |
| Inverter | Delta, Taiwan |  |  |  |
| Feeding Speed (m/min) | 16 |  |  |  |  |
| Uncoiler Motor | Non-motorized |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| **4. GL-H high precison for material thickness 0.5-4.5mm** |  |  |  |
|  |  |  |  |  |  |
| **Model** | **GL-300H** | **GL-400H** | **GL-500H** | **GL-600H** |  |
| Coil Width (mm) | 300 | 400 | 500 | 600 |  |
| Coil Thickness (mm) | 0.5-4.5 |  |  |  |  |
| Coil I.D. (mm) | 460-520 |  |  |  |  |
| Coil O.D. (mm) | 1200 |  |  |  |  |
| Loading Capacity (kgs) | 2000 | 2000 | 2000 | 5000 |  |
| Expansion | Manual |  |  |  |  |
| Straightener Roller | Ø68mm\*7pcs |  |  |  |  |
| Straightener Motor  | 2.2kW | 2.2kW | 4.4kW | 4.4kW |  |
| Roller Pressing  | Pneumatic Rod |  |  |  |
| Roller Adjustment | Eccentric turbine worm adjusting |  |  |
| Inverter | Delta, Taiwan |  |  |  |
| Feeding Speed (m/min) | 16 |  |  |  |  |
| Uncoiler Motor | 1.5kW | 1.5kW | 1.5kW | 2.2kW |  |
|  |  |  |  |  |  |
| Please contact with our sales team to find a suitable configuration for your material: |
| Email: export@he-machine.com |  |  |  |  |
| Tel: +86 755 28372363 |  |  |  |  |  |
| Add: F1601-02, A4 Bldg Zhujiang Plaza, Longgang, Shenzhen, 518172, China |
| www.hongerjixie.com    |  |  |  |  |  |