|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **HONGER SHEET METAL STRAIGHTENER** | | |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **1. TL Straightener for material thickness 0.4-2.2mm** | | | | |  |  |  |
|  |  |  |  |  |  |  |  |
| **Model** | **TL-200** | **TL-300** | **TL-400** | **TL-500** | **TL-600** | **TL-700** | **TL-800** |
| Coil Width (mm) | 200 | 300 | 400 | 500 | 600 | 700 | 800 |
| Coil Thickness (mm) | 0.4-2.2 |  |  |  |  |  |  |
| Straightening Roller | Ф50\*7 |  | Ф60\*7 |  |  |  |  |
| Feeding Roller | Ф60\*2, Ф80\*2 | | Ф70\*2, Ф98\*2 | |  |  |  |
| Power (HP) | 1 |  | 2 |  | 3 |  | 5 |
| Inverter | No |  |  |  |  |  |  |
| Feeding Speed (m/min) | 16 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **2. HS-A High Precision Straightener for material thickness 0.5-4.5mm** | | | | | | |  |
|  |  |  |  |  |  |  |  |
| **Model** | **HS-300A** | **HS-400A** | **HS-500A** | **HS-600A** |  |  |  |
| Coil Width (mm) | 300 | 400 | 500 | 600 |  |  |  |
| Coil Thickness (mm) | 0.5-4.5 |  |  |  |  |  |  |
| Straightening Roller | Ø70\*9 |  |  |  |  |  |  |
| Feeding Roller | Ø95\*4 |  |  |  |  |  |  |
| Roller Pressing Way | Cylinder Pressure | | |  |  |  |  |
| Roller Adjustment | Eccentric turbine worm adjusting | | | |  |  |  |
| Power (HP) | 5 |  | 7.5 |  |  |  |  |
| Inverter | Delta, Taiwan | |  |  |  |  |  |
| Feeding Speed (m/min) | 16 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **3. HS-B High Precision Straightener for material thickness 1.0-6.0mm** | | | | | | |  |
|  |  |  |  |  |  |  |  |
| **Model** | **HS-300B** | **HS-400B** | **HS-500B** | **HS-600B** |  |  |  |
| Coil Width (mm) | 300 | 400 | 500 | 600 |  |  |  |
| Coil Thickness (mm) | 1.0-6.0 |  |  |  |  |  |  |
| Straightening Roller | Ø90\*9 |  |  |  |  |  |  |
| Feeding Roller | Ø120\*4 |  |  |  |  |  |  |
| Roller Pressing Way | Cylinder Pressure | | |  |  |  |  |
| Roller Adjustment | Eccentric turbine worm adjusting | | | |  |  |  |
| Power (HP) | 5 |  | 7.5 |  |  |  |  |
| Inverter | Delta, Taiwan | |  |  |  |  |  |
| Feeding Speed (m/min) | 16 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **4. High Speed S-loop Straightener** | | |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **Model** | **JMS-200** |  | **JMS-300** |  |  |  |  |
| Coil Width (mm) | 200 |  | 300 |  |  |  |  |
| Coil Thickness (mm) | 0.3-1.2 |  |  |  |  |  |  |
| Straightening Roller | Ø32\*15 |  |  |  |  |  |  |
| Roller Adjustment | 4 points adjusting | |  |  |  |  |  |
| Transmission Way | Bottom gear drive | |  |  |  |  |  |
| Power (HP) | 1 |  |  |  |  |  |  |
| Inverter | No |  |  |  |  |  |  |
| Feeding Speed (m/min) | 16 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **5. High Precision Straightener SNL for material thickness 0.1-0.6mm** | | | | | | |  |
|  |  |  |  |  |  |  |  |
| **Model** | **SNL-150** | **SNL-200** | **SNL-300** | **SNL-400** |  |  |  |
| Coil Width (mm) | 150 | 200 | 300 | 400 |  |  |  |
| Coil Thickness (mm) | 0.1-0.6 |  |  |  |  |  |  |
| Straightening Roller | Ø20\*19 |  |  |  |  |  |  |
| Roller Adjustment | 4 points adjusting | |  |  |  |  |  |
| Transmission Way | Bottom gear drive | |  |  |  |  |  |
| Power (HP) | 0.5 |  | 1 |  |  |  |  |
| Inverter | No |  |  |  |  |  |  |
| Feeding Speed (m/min) | 16 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| Please contact with our sales team to find a suitable configuration for your material: | | | | | | | |
| Email: export@he-machine.com | |  |  |  |  |  |  |
| Tel: +86 755 28372363 |  |  |  |  |  |  |  |
| Add: F1601-02, A4 Bldg Zhujiang Plaza, Longgang, Shenzhen, 518172, China | | | | | | |  |
| www.hongerjixie.com | |  |  |  |  |  |  |