|  |
| --- |
| **HONGER GLK SERIES COIL FEEDING LINE** |
|
| **1. GLK2 for coil thickness 0.3-3.2mm** |  |  |  |  |  |
| Model | GLK2-400 | GLK2-500 | GLK2-600 | GLK2-800 | GLK2-1000 |  |
| Material Yield Strength (N/mm²) | ≤245 |  |
| Material Tensile Strength | ≤392 |  |
| Coil Width (mm) | 50-400 | 50-500 | 50-600 | 50-800 | 50-1000 |  |
| Coil Thickness (mm) | **0.3-3.2** |  |
| Feeding Length (mm) | 9999.99 |  |
| Coil I.D. (mm) | Φ480-Φ520 |  |
| Coil O.D. (mm) | Φ1200 |  |
| Max. Coil Weight (kgs) | 3000 | 3000 | 5000 | 5000 | 7000 |  |
| Feeding Speed (m/min) | 16-24 |  |
| Feeding Precision | ±0.1mm |  |
| Straightener Roller | Φ48mm\*11pcs | Φ68mm\*7pcs Up4/Down3 |  |
| Feeding Roller | Φ68mm\*2pcs | Φ88mm\*2pcs |  |
| Auxiliary Roller | N/A |  |
| Pressing Arm | Pneumatic Type |  |
| Uncoiler Motor | 1.5kw | 1.5kw | 2.2kw | 2.2kw | 3.7kw |  |
| Servo Motor | 2.9kw | 2.9kw | 2.9kw | 4.4kw | 5.5kw |  |
| Feeding Line Heght | Motor-driven ,Feeding line height ± 100mm |  |
| Expansion | Hydraulic  |  |
| Feeding Direction  | L→R |  |
| Pneumatic Pressure | 0.5Mpa |  |
| Uncoiling Direction | Counterclockwise |  |
| Hydraulic Pressure  | 70 kg/mm² |  |
|  |  |  |  |  |  |  |
| **2. GLK3 for coil thickness 0.5-4.5mm** |  |  |  |  |  |
| Model | GLK3-400 | GLK3-500 | GLK3-600 | GLK3-800 | GLK3-1000 | GLK3-1300 |
| Material Yield Strength (N/mm²) | ≤245 |
| Material Tensile Strength | ≤392 |
| Coil Width (mm) | 70-400 | 70-500 | 70-600 | 70-800 | 70-1000 | 70-1300 |
| Coil Thickness (mm) | **0.5-4.5** |
| Feeding Length (mm) | 9999.99 |
| Coil I.D. (mm) | Φ480-Φ520 |
| Coil O.D. (mm) | Φ1200 |
| Max. Coil Weight (kgs) | 3000 | 3000 | 5000 | 5000 | 7000 | 10000 |
| Feeding Speed (m/min) | 16-24 |
| Feeding Precision | ±0.15mm |
| Straightener Roller | Φ68mm\*7pcs Up4/Down3 |
| Feeding Roller | Φ88mm\*2pcs |
| Auxiliary Roller | N/A | N/A | N/A | 1group | 2groups | 3groups |
| Pressing Arm | Pneumatic Type |
| Uncoiler Motor | 1.5kw | 1.5kw | 2.2kw | 2.2kw | 3.7kw | 5.5kw |
| Servo Motor | 4.4kw | 4.4kw | 4.4kw | 5.5kw | 5.5kw | 7.5kw |
| Feeding Line Heght | Motor-driven ,Feeding line height ± 100mm |
| Expansion | Hydraulic  |
| Feeding Direction  | L→R |
| Pneumatic Pressure | 0.5Mpa |
| Uncoiling Direction | Counterclockwise |
| Hydraulic Pressure  | 70 kg/mm² |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
| **3. GLK4 for coil thickness 0.6-6.0mm** |  |  |  |  |  |
| Model | GLK4-400 | GLK4-500 | GLK4-600 | GLK4-800 | GLK4-1000 | GLK4-1300 |
| Material Yield Strength (N/mm²) | ≤245 |
| Material Tensile Strength | ≤392 |
| Coil Width (mm) | 70-400 | 70-500 | 70-600 | 70-800 | 70-1000 | 70-1300 |
| Coil Thickness (mm) | **0.6-6.0** |
| Feeding Length (mm) | 9999.99 |
| Coil I.D. (mm) | Φ508 |
| Coil O.D. (mm) | Φ1400 |
| Max. Coil Weight (kgs) | 5000 | 5000 | 5000 | 7000 | 7000 | 10000 |
| Feeding Speed (m/min) | 16-24 |
| Feeding Precision | ±0.15mm |
| Straightener Roller | Φ68mm\*7pcs Up4/Down3 |
| Feeding Roller | Φ88mm\*2pcs |
| Auxiliary Roller | 3groups |
| Pressing Arm | Pneumatic Type |
| Uncoiler Motor | 2.2kw | 2.2kw | 2.2kw | 3.7kw | 3.7kw | 7.5kw |
| Servo Motor | 5.5kw | 5.5kw | 7.5kw | 7.5kw | 11kw | 11kw |
| Feeding Line Heght | Motor-driven ,Feeding line height ± 100mm |
| Expansion | Hydraulic  |
| Feeding Direction  | L→R |
| Pneumatic Pressure | 0.5Mpa |
| Uncoiling Direction | Counterclockwise |
| Hydraulic Pressure  | 70 kg/mm² |
|  |  |  |  |  |  |  |
| **4. GLK-H for high strength material**  |  |  |  |  |  |
| Please contact with our sales team to find a suitable configuration for your high strength material: |  |  |
| Email: export@he-machine.com |  |  |  |  |  |  |
| Tel: +86 755 28372363 |  |  |  |  |  |  |
| Add: F1601-02, A4 Bldg Zhujiang Plaza, Longgang, Shenzhen, 518172, China |  |  |  |
| www.hongerjixie.com    |  |  |  |  |  |  |