Product introduction:

Suitable for electrical products, lamps, electrical cabinets, electrical components, communications products, automobiles, motorcycles and spare parts, outdoor lighting and signal devices and other products to do waterproof performance testing and IP waterproof rating test.

Technical Parameter:

|  |  |
| --- | --- |
| **Model** | **DTK-E710-4** |
| Internal dimension | Diameter 606 \* height 1000mm | Diameter 820 \* height 1500mm |
| External dimension | Diameter 820 \* height 2000mm | Diameter 1000 \* height 2000mm |
| Chamber material | 304, thickness 3mm |
| Water pressure | 0 ~ 0.5MPa adopt air compressor |
| Test duration | 0 ~ 99min, 99sec |
| Sample lift device | Portable stainless steel basket |
| Water level display | Water pipe with scale  |
| Controller | Digital pressure gauge & timer |
| Power source | Three phase, AC380V, 50/60HZ |