Product introduction:

UV Weathering Test Chamber can simulate the sun, rain spray and condensation resulting damage to test the materials by exposure to sunlight with moisture and temperature.

This test machine can get the results of damage after several days or weeks which is equal to expose to outside for a few months. The damages include fading, discoloration, brightness down, powder, crack, blur, brittle, strength decreases and oxidation. It provides the reference with testing data for improvement of existing materials, or to assess the impact of changes in product durability and other aspects.

Production parameters:

|  |  |  |
| --- | --- | --- |
| Model | DTK-UVADTK-UVB | DTK-UVADTK-UVB |
| Internal chamber design | standard chamber | Flat type chamber |
| Internal dimension(W\*D\*H) | N/A | 1140\*650\*500 mm |
| External dimension (W\*D\*H) | 1300\*500\*1460 mm | 1340\*700\*1800 mm |
| Temperature range | RT~ 70℃ |
| Temperature fluctuation | ±2℃ |
| Internal & External chamber material | Stainless steel 304 |
| Control system | Programmable controller, LCD touch screen Illumination, condensation and water spray test cycles are programmable |
| UV lamp | Atlas UV-A: 315-400nm/ UV-B: 380-315nm (8pcs, 1200h lifetime) |
| Irradiance meter | 0.45~0.85W/cm2 can be adjusted (Optional) |
| Distance from sample to lamp | 50±2mm |
| Sample dimension (Standard chamber) | 75×290mm (24pcs) or 75x150mm (48pcs), max. thickness 5mm |
| Sample dimension (Flat type chamber) | Irregular test samples |
| Power | Single phase ,AC 220V 50/60HZ |

Function:

Meet Specifications

\* Meet customer requirements

\* Stay ahead of government regulations

Prevent Field Failures

\* Improve quality and durability

\* Enhance reputation

\* Assure product performance

Gain a Competitive Edge

\* Save on material costs

\* Expand product lines

\* Enter new markets

\* Outrun the competition

**design criteria:General:**

•ASTM G151

• ASTM G154

**Coating:**

• ASTM D3794

• ASTM D4587

• ISO 11507

• ISO 20340

**Adhesive:**

• ASTM C1184

• ASTM C1442

• ASTM D904

• ASTM D5215

**Plastic:**

• ASTM D4329

• ASTM D4674

• ASTM D5208

• ASTM D6662

• ISO 4892-3 …

|  |
| --- |
| Q-test Controller |
| Programmable LCD controller, can do cyclic test with temp, humid, water spray and condensation. |
| UV lamps |
| UV-A and UV-B lamps for option |
| Sample Holder |
| Test specimens are mounted on both the front and back side of the UV Tester, providing a large sample capacity.Sample holder can be customized. |