Product Description:

一、Use:

Drying box is mainly used for baking, drying, heat treatment and heating. Industrial and agricultural production, scientific research, health care and other units can be used in the laboratory, but not suitable for volatile substances, flammable materials, so as not to cause an explosion.

二、Working principle

This machine adopts the thin steel plate is made in the studio sample shelf, an insulation layer between the studio and the studio at the bottom of the box body casing and is provided with an air hole, cold air from the bottom into the box, discharged from the top row of holes, two sets of heating components distributed in the lower part of the studio. Use as needed,

The temperature by the temperature sensor and temperature control control. The constant temperature system, the fuse is installed on the left side of the box body and has a movable door device, and the maintenance is convenient.

Technical Parameter:

|  |  |  |  |
| --- | --- | --- | --- |
| Model | DTK-DO-25 | DTK-DO-35 | DTK-DO-45 |
| Internal dimension  WxHxD | 250\*250\*250 | 350\*350\*350 | 350\*350\*350 |
| External dimensionWxHxD | 460\*490\*450 | 570\*650\*520 | 450\*450\*500 |
| Model | DTK-DO-55 | DTK-DO-75 | DTK-DO-100 |
| Internal dimension  WxHxD | 550\*550\*450 | 600\*750\*500 | 100\*1600\*600 |
| External dimensionWxHxD | 730\*840\*670 | 880\*930\*720 | 1140\*2150\*800 |
| Power supply | AC220V/50HZ | | |
| Temperature range | RT+10-250℃ | | |
| Temperature control accuracy | ±1℃ | | |
| power | 2200W | | |
| Weight | 120KG | | |
| Sample tray | 3 Block（3 layer） | | |
| Alarm range | 1~9999min | | |