CONCRETE PUMP SINGLE WALL ELBOW

|  |
| --- |
| CONCRETE PUMP SINGEL WALL ELBOW:DN125\*R275\*90D  |
| ID(Inner Diameter) | OD(Outer Diameter) | Thickness(mm) | Bend radius  | Collar size | Material | Weight(Kgs) | Service life |
| 125mm | 140mm |  11-12mm  | R275 | Sk148mm | Mn13 | 16kgs | 30000 |
| Backend Arc thickness: 14mm  |
| CONCRETE PUMP SINGLE WALL ELBOW:DN125\*R275\*45D  |
| ID(Inner Diameter) | OD(Outer Diameter) | Thickness(mm) | Bend radius |  Collar size | Material | Weight(Kgs) | Service life |
| 125mm | 140mm |  11-12mm  | R275 | Sk148mm | Mn13 | 9kgs | 30000 |
| Backend Arc thickness: 14mm  |

CONCRETE PUMP DOUBLE LAYER ELBOW

|  |
| --- |
| CONCRETE PUMP TWIN WALL ELBOW:DN125\*R275\*90D |
| ID(Inner Diameter) | OD(Outer Diameter) | Thickness(mm) | Bend radius | Collar size | Material | Weight(Kgs) | Service life |
| 125mm | 140mm | Inner elbow thickness:10-11mm  | R275  | Sk148mm  | Inner elbow :Alloy steel  | 16 | 50000cbm |
| Outer elbow thickness:3-4mm | Outer elbow: Q235 |
| Ending collar thickness:7-8mm |
| CONCRETE PUMP TWIN WALL ELBOW:DN125\*R275\*45D |
| ID(Inner Diameter) | OD(Outer Diameter) | Thickness(mm) | Bend radius | Collar size | Material | Weight(Kgs) | Service life |
| 125mm | 140mm  | Inner elbow thickness:10-11mm  | R275  | Sk148mm  | Inner elbow :Alloy steel  | 9 | 50000cbm |
| Outer elbow thickness:3-4mm | Outer elbow: Q235 |
| Ending collar thickness :7-8mm |