
**paper preheater triple preheater**



ⅰ、Structural features：

★The preheating roller is designed with butterfly head, which conforms to the first class national standard of pressure vessel and has the certificate of pressure vessel.

★The roll surface after precision grinding, fine grinding and hard chromium plating processing，surface friction is small and durable。

★Electric adjustment wrap angle , wrap angle can be rotated within 360 °to adjust the paper heat area .

★The double-stage reducer is used to adjust the angle of the package and has the function of self-locking.

ⅱ、Technical parameter：

★Effective width：1800mm

★Diameter of the preheat roller：￠600mm

★Diameter of the angle：￠85mm×2

★Steam temperature：150-200 ℃

★Steam pressure：0.8-1.3Mpa

★Motor power：250W short（S2）work system