**DMT-120paper sheet delivery and side conveyor**



ⅰ、Structural features：

★Adopted on the 16th channel welded。Electric adjustment of cardboard the size of the lateral output pneumatic control board, electrically adjustable conveyor speed.

★Cardboard sheets to the desired number or height requirements will be controlled by a foot switch out of cardboard。

★Vertical bin using wide flat belt conveyor transport。

ⅱ、Technical parameter：

★The maximum accumulation length：3000mm

★The maximum stack height：200mm

ⅲ、Powered motor parameters：

★Main conveyor motor：3Kw adopt frequency motor

★Lateral output of the motor：1.5Kw Three-phase asynchronous motor

★Walking Motor：1.5Kw Three-phase asynchronous motor