**Automatic paper picking machine**

****

ⅰ、Structural features：

★Maximum diameter of base paper：1500mm。

★Mill roll stand with automatic tension control, high-speed paper receiving success rate.

★Paperless tail then the paper, to reduce the paper loss(Paper tape and only partially overlap with a width of 40mm.)

★When the paper car out, automatic transfer out,and the vacuum suction,easy paper loading, automatic tension control,zero error of paper receiving.

★all PLC automatic control,accurate,less failure,easy maintenance.

★The first buffer wheel pull the paper, automatic alignment, easy to pull paper.

★Machine superiority, cylinder control of the paper machine at high speed, the paper will not appear in the ordinary motor control of broken tiles, foaming phenomenon.

★Maximum paper speed 150 m / min.

ⅱ、Technical parameter：

1. Effective width：1800mm

2、Operation direction：left or right（determined in accordance with customer plant）

3、Design speed：150m/min

4、Working speed：0-150m/min

5、Pressure：6bpa

6、Single machine weight：max 2300Kg

ⅲ、Roller diameter parameter：

1. Up guide paper shaft：￠126mm
2. Down guide paper guide： ￠126mm
3. Buffer roller guide roller1： ￠118mm
4. Buffer roller guide roller2：￠126mm
5. Paper pinch roll： ￠99mm
6. Paper roll：￠99mm