**SHANGHAI JINYUAN PLASTIC PRODUCTS CO.,LTD**

**Product Description**

The difference between the three materials，PP/PET/PVC

PP：（Our factory production）

化学名称：聚丙烯，英文:Polypropylene（简称PP）

材质性能：环保、无毒 、无味、耐高温、耐腐蚀、不易撕裂、韧性好，透明度比PVC和PET低，重量轻，PP比重0.91。

用途：适合做各式文件夹、手提袋、包装盒、垫板、笔记本封面等

PVC：（Divided into two，soft PVC and hard PVC）Materials purchased Chemical Name: PVC, English: Polyvinyl chloride (referred to as PVC)Material Properties: Rigid PVC is not environmental protection, transparency, high ratio of PP, hard material not easily deformed, has good tensile, flexural, compressive strength, specific gravity of 1.40.

Soft PVC can be divided Cape permeability, ultra-transparent, environmental protection and not environmentally friendly, soft and strong, specific gravity of 1.40.

Uses: hard material suitable for packaging, cards, and other OEM.

Soft material suitable slipcase, zipper bags, card sets, book bags, all kinds of leather bags and so on.

PET：Materials purchased Chemical name: polyethylene terephthalate English: Polythylene terephthalate (abbreviated PET)

Material properties: environmentally friendly, non-toxic, tasteless, good temperature, low temperature performance, impact strength is 3-5 times that of other materials, folding is good. Transparent, hard material not easily deformed, specific gravity 1.40

Uses: suitable for pallets, bottles, lunch boxes, high-end cosmetics packaging, etc.

Cost Structure

Customers asked us a product, the six points we need to know:

1. What kind of material and thickness

2. Printing colors

3. The process, after

4. Packing

5. The number of

6. quotations (RMB, US gold / FOB / CIF / CNF, etc.)

The basic structure of costs: printing materials + + + package, after + accessories + shipping

Materials: Expand the area + 1cm bleed.

Printing: CMYK or spot color printing (less than the price of 3,000 large sheet of printing costs are the same)

After said: die cutting, pressing, ultrasonic, nail Sihetun deduction, nail clips, etc.

Accessories: Commonly used materials with instructions, labels, OPP bags

package:

Freight:

**1. File folder**

**E310 file folder**

|  |  |
| --- | --- |
| **Product name：** | **E310 file folder/L shape file folder** |
| Material： | Environmental mirror PP, Cape through |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 310\*220  460\*640----2 piece |
| Material thickness（mm）： | 0.2 |
| Product Weight（g）： | 22.5 |
| printing art： | CMYK+white Offset printing ink in printing |
| Production Process： | Produced films - Printing - die - Ultrasound - Packaging |



**3 in file folder**

|  |  |
| --- | --- |
| **Product name：** | **3 in file folder** |
| Material： | Environmental mirror PP, Cape through |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 310\*220  460\*640----1 piece |
| Material thickness（mm）： | 0.2 |
| Product Weight（g）： | 48.4 |
| Printing art： | Cover and inside pages are  CMYK + white offset printing, ink is printed inside |
| Production Process： | Produced films - Printing - die - Ultrasound - Packaging |



**4 in file folder**

|  |  |
| --- | --- |
| **Product name：** | **4 in file folder** |
| Material： | Environmental mirror PP, Cape through |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 310\*220  460\*640--1piece，320\*230---1 piece |
| Material thickness（mm）： | 0.2 |
| Product Weight（g）： | 58.5 |
| printing art： | Cover and inside pages are  CMYK + white offset printing, ink is printed inside |
| Production Process： | Produced films - Printing - die - Ultrasound - Packaging |



**5 in file folder**

|  |  |
| --- | --- |
| **Product name：** | **5 in file folder** |
| Material： | Environmental mirror PP, Cape through |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 310\*235  480\*645-----2 piece |
| Material thickness（mm）： | 0.2 |
| Product Weight（g）： | 74.8 |
| printing art： | Front and back covers CMYK + white offset  Ink in print, in the page does not print |
| Production Process： | Produced films - Printing - die - Ultrasound - Packaging |



**10 in file folder**

|  |  |
| --- | --- |
| **Product name：** | **10 in file folder** |
| Material： | Environmental mirror PP, front and back covers of Cape transparent material, inside color material |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 310\*235  490\*650------2 piece |
| Material thickness（mm）： | 0.2 |
| Product Weight（g）： | 154 |
| printing art： | Front and back covers CMYK + white offset  Ink in print, in the page does not print |
| Production Process： | Produced films - Printing - die - Ultrasound - Packaging |




**File folder with a zipper**

|  |  |
| --- | --- |
| **Product name：** | **File folder with a zipper** |
| Material： | Environmental mirror PP, front and back covers Cape thoroughly, inside color |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 310\*235  490\*650------2 piece |
| Material thickness（mm）： | 0.2 |
| Product Weight（g）： | 103.5 |
| printing art： | Front and back covers CMYK + white offset  Ink in print, in the page does not print |
| Production Process： | Produced films - Printing - die - pressed zipper - hot - Ultrasound - Packaging |



**Open type 5 in folder**

|  |  |
| --- | --- |
| **Product name：** | **Open type 5 in folder** |
| Material： | Environmental protection PP mirror cover, transparent material, color pages |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 310\*240  920\*650------2 piece |
| Material thickness（mm）： | 0.2 |
| Product Weight（g）： | 103.5 |
| printing art： | Front and back covers CMYK + white offset printing ink in printing, printing on the boot |
| Production Process： | Produced films - Printing - die - Ultrasound - Packaging |



**Powerful folder**

|  |  |
| --- | --- |
| **Product name：** | **Powerful folder** |
| Material： | Green frosted PP, material qualities |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 310\*240\*20  520\*640----2 piece |
| Material thickness（mm）： | 0.8 |
| Product Weight（g）： | 140 |
| printing art： | 1 color screen printing |
| Production Process： | Produced films - Printing - die - Nail jig - Packaging |



**Loose-leaf binder**

|  |  |
| --- | --- |
| **Product name：** | **Loose-leaf binder** |
| Material： | Environmental protection double-sided matte PP, translucent green |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 310\*240\*40  540\*640----2 piece |
| Material thickness（mm）： | 0.92 |
| Product Weight（g）： | 168.2 |
| printing art： | gilding |
| Production Process： | Products - stamping die cutting nail fixture - pressure - packing strap |



**2. File package**

**Loose-leaf binder**

|  |  |
| --- | --- |
| **Product name：** | **File package** |
| Material： | Environmental protection double-sided matte PP (metal blue) |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 318\*238\*40  420\*720----1 piece |
| Material thickness（mm）： | 0.5 |
| Product Weight（g）： | 89 |
| printing art： | Bronzing LOGO |
| Production Process： | Produced films - stamping - die - stick Velcro - ultrasonic - Packaging |



**File package**

|  |  |
| --- | --- |
| **Product name：** | **File package** |
| Material： | Environmental sided matte PP, white |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 323\*240\*40  680\*420----1 piece |
| Material thickness（mm）： | 0.81 |
| Product Weight（g）： | 187.4 |
| printing art： | Offset CMYK + white, is printed |
| Production Process： | Produced films - Printing - die - clinch - Ultrasound - Packaging |



**File package**

|  |  |
| --- | --- |
| **Product name：** | **File package** |
| Material： | Environmental sided matte PP, Cape transparent material |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 310\*245 |
| Material thickness（mm）： | 0.46 |
| Product Weight（g）： | 90 |
| printing art： | CMYK + white offset printing ink in printing |
| Production Process： | Produced films - Printing - die - wear elastic band - Packaging |



**3. Material bag**

|  |  |
| --- | --- |
| **Product name：** | **Material bag** |
| Material： | Environmental mirror PP, Cape transparent material |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size（mm）： | 344\*250\*30 |
| Material thickness（mm）： | 0.2 |
| Product Weight（g）： | 37.8 |
| printing art： | CMYK + white offset printing ink in printing |
| Production Process： | Produced films - Printing - die - pressed zipper - hot - Nail Corner - Packaging |



**4.Information Booklet**

**Information Booklet**

|  |  |
| --- | --- |
| **Product name：** | **Information Booklet** |
| Material： | Environmental sided matte PP, white material |
| Product Specifications： | B5 |
| Product Size（mm）：  In-page size（mm）：  Expand Size (mm): | 235\*160\*10  320\*227mm  380\*500\*0.6-----2 piece |
| Material Thickness (mm):  Inside Thickness (mm): | 0.6  Single 0.4 |
| Product Weight (g): | 64.4 |
| printing art: | CMYK + white offset printing, ink is printed |
| Production process: | Produced films - Printing - die - Ultrasonic inside pages - Packaging |



**Information Booklet**

|  |  |
| --- | --- |
| **Product name：** | **Information Booklet** |
| Material： | Environmental sided matte PP, translucent blue |
| Product Size（mm）：  In-page size（mm）：  Expand Size (mm): | 315 \* 235 \* 16,  471 \* 315 \* 20  650 \* 505 ---- 2 fight |
| Material Thickness (mm):  Inside Thickness (mm): | 0.65mm  Single 0.04mm |
| Product Weight (g): | 194.4 |
| printing art: | CMYK + white offset printing ink in printing |
| Production process: | Produced films - Printing - die - Ultrasonic inside pages - Packaging |



**Information Booklet**

|  |  |
| --- | --- |
| **Product name：** | **Information Booklet** |
| Material： | Environmental sided matte PP, translucent blue |
| Product Size（mm）：  In-page size（mm）：  Expand Size (mm): | 319 \* 235 \* 15  505 \* 670 ---- 2 fight  47.1 \* 319 (20-page) |
| Material Thickness (mm):  Inside Thickness (mm): | 0.61  8 double wire |
| Product Weight (g): | 168.2 |
| printing art: | No printing |
| Production process: | Produced films - Printing - die - Ultrasonic inside pages - Packaging |



**5.Slipcase**

|  |  |
| --- | --- |
| **Product name：** | **Slipcase** |
| Material： | Environmental mirror PP, Cape through |
| Product Specifications： | B5 |
| Product Size（mm）：  Expand Size（mm）： | 220 \* 155  490 \* 690 ----- 3 fight |
| Material thickness（mm）： | 0.17 |
| Product Weight（g）： | 16.4 |
| printing art： | CMYK + white offset printing ink in printing |
| Production Process： | Produced films - Printing - die - Ultrasound - Packaging |



**6.Expanding File**

|  |  |
| --- | --- |
| **Product name：** | **Organ bags, Georgia 12PP** |
| Material： | Green frosted PP, transparent |
| Product Specifications： | A4 |
| Product Size（mm）：  Expand Size (mm): | 310\*240\*30  720\*330---1 piece |
| Material Thickness (mm):  Inside Thickness (mm): | 0.6  0.2 |
| Product Weight (g): | 288 |
| Printing art: | CMYK + white offset printing ink in printing |
| Production Process | Produced films - Printing - die - a combination of internal pockets - hot - Ultrasound - clinch - wear elastic band - Packaging |



**Suede organ package**

|  |  |
| --- | --- |
| **Product name：** | **Suede organ package** |
| Material： | Suede + cardboard + green PP |
| Product Specifications： | A4 |
| Product Size（mm）： | 220 \* 155 |
| Material thickness（mm）： | 0.2 |
| Product Weight（g）： | 603.6 |
| printing art： | No |
| Production Process： | Produced films - die - a combination of inside pages - sewing - the buckle - Packaging |



**7.Tag**

|  |  |
| --- | --- |
| **Product name：** | **Tag** |
| Material： | White PVC |
| Product Specifications： |  |
| Product Size（mm）：  Expand Size (mm): | 200\*110  430\*250---4 |
| Material thickness（mm）： | 1.17 |
| Product Weight（g）： | 44.8 |
| printing art： | 4 color screen printing (two sided printing) |
| Production Process： | Film production - Printing - die - cutting - packaging |

![D{NU{%GRX](ZORDJ%18TW]L](data:image/jpeg;base64,)

**Tag**

|  |  |
| --- | --- |
| **Product name：** | **Tag** |
| Material： | Green black matte PP |
| Product Specifications： |  |
| Product Size（mm）：  Expand Size (mm): | 200\*110  510\*230---4 |
| Material thickness（mm）： | 0.75 |
| Product Weight（g）： | 14.2 |
| printing art： | 1 color screen printing |
| Production Process： | Film production - Printing - die - cutting - packaging |



**Tag**

|  |  |
| --- | --- |
| **Product name：** | **Tag** |
| Material： | Environmental protection double-sided matte PP (a variety of colors) |
| Product Specifications： |  |
| Product Size（mm）：  Expand Size (mm): | 400\*90  420\*400---4 |
| Material thickness（mm）： | 1.2 |
| Product Weight（g）： | 36.8 |
| printing art： | 1 color screen printing |
| Production Process： | Film production - Printing - die - cutting - packaging |



**8. Name-card album**

|  |  |
| --- | --- |
| **Product name：** | **Name-card album** |
| Material： | Environmental sided matte PU, white material |
| Product Specifications： |  |
| Product Size（mm）：  Expand Size (mm): | 214\*108\*20  500\*460----4 |
| Material Thickness (mm):  Inside Thickness (mm): | 0.68  Double 10 wire \* 8 |
| Product Weight (g): | 71.4 |
| Printing art: | CMYK + white offset printing ink in printing |
| Production Process | Produced films - Printing - die - Ultrasound - Packaging |



**9. Portable Notebook**

|  |  |
| --- | --- |
| **Product name：** | **Portable Notebook** |
| Material： | Environmental sided matte PP, white material |
| Product Specifications： |  |
| Product Size（mm）：  Expand Size (mm): | 305\*175\*6 |
| Material thickness（mm）： | 0.4 |
| Product Weight（g）： | 218 |
| printing art： | CMYK + white offset printing, ink is printed |
| Production Process： | Produced films - Printing - die - Loading and coil - loaded handle - Packaging |



|  |  |
| --- | --- |
| **Product name：** | **Portable Notebook** |
| Material： | Environmental sided matte PP, white material |
| Product Specifications： |  |
| Product Size（mm）：  Expand Size (mm): | 280\*217\*6 |
| Material thickness（mm）： | 0.52 |
| Product Weight（g）： | 240 |
| printing art： | CMYK + white offset printing, ink is printed |
| Production Process： | Produced films - Printing - die - Loading and coil - loaded handle - Packaging |



**Golden Notebook**

|  |  |
| --- | --- |
| **Product name：** | **Golden Notebook** |
| Material： | Environmental sided matte PP, golden material |
| Product Specifications： |  |
| Product Size（mm）：  Expand Size (mm): | 170\*190\*35 |
| Material thickness（mm）： | Notebook Cover 1.2  Envelope 0.7 |
| Product Weight（g）： | 476.5 |
| printing art： | No |
| Production Process： | Produced films - Printing - die - Loading and coil - loaded handle - Packaging |



**Pencil box**

|  |  |
| --- | --- |
| **Product name：** | Pencil box |
| Material： | Environmental protection double-sided matte PP |
| Product Specifications： |  |
| Product Size（mm）：  Expand Size (mm): | 200\*80\*28 |
| Material thickness（mm）： | Carton: 0.47, inside the box: 0.6 |
| Product Weight（g）： | 37.2 |
| printing art： | Offset CMYK + White |
| Production Process： | Produced films - Printing - die - Ultrasound - clinch - Packaging |



Ruler

|  |  |
| --- | --- |
| **Product name：** | Ruler |
| Material： | White PVC |
| Product Specifications： |  |
| Product Size（mm）：  Expand Size (mm): | 160\*40  250\*350----10 |
| Material thickness（mm）： | 0.6 |
| Product Weight（g）： | 6 |
| printing art： | CMYK + white offset printing, ink is printed |
| Production Process： | Produced films - Printing - die - Packaging |



