**1. What should the factors pay attention to when chooses a plastic tarpaulin?**

With the increasing demand for plastic tarpaulin, now, more and more customers began to engage in the production and sales of plastic tarpaulin in our market. In this case, there are excellent manufacturers, but also there have been some bad business. So what should we pay attention to when choosing the product? Let’s follow the editor to look at it.

A: First of all, check the latitude and longitude of the tarp product. The denser, the better quality of the product is.

B: Carefully check its waterproof; you can try to shower the surface of the product with a small amount of water. If the tarp is not wet by water, it shows that its quality is good.

C: Secondly, we also need to pay attention to the roughness of the product surface. You can feel the roughness and softness of the product by your hand.

**2. Fireproof tarpaulins ensure the safety of goods in transit.**

 Fireproof tarpaulin as its name is a kind of fire prevention function of tarpaulin. It ensures the safety of goods in transit, which can delay the burning time of the dangerous goods and precision instruments. Therefore, the product is used by many chemical industries. Here I will introduce some characteristics of the fireproof tarpaulin to you.

The use of fireproof tarpaulin can well- protect the object from the heat and spark zone, and completely prevent the combustion or isolation combustion. As the cover canopy has a heat insulation function, which can delay the explosion time of dangerous goods or precision instruments. And thus we have the chance to find the risks and rescue on time.

Cover tarpaulin used in flammable and explosive dangerous goods and precision instruments and equipment production, storage, transportation for the security protection.

When we use the product, dangerous goods and precision instruments and equipment should be completely covered, so that it can reduce the combustion and explosion case affected by small -mars.

**3. You need to pay attention to some small details for the maintenance of waterproof tarpaulin.**

In general, the environment that we use the tarpaulin is relatively poor, which is a great harm to waterproof tarpaulin. In order to extend the service life of waterproof tarpaulin, then which problems do you need to pay attention to in the maintenance of the product? Let’s follow the editor to look at It.

1. You should receive carefully the parts of tarpaulins after use it to avoid the loss , or the next time you do not know where the parts go.

 2, when storing tarpaulin, you need to avoid sharp objects in order to avoid scratches, scratches, which Is not conducive to use in the future.

  3, Reading carefully the instructions when finished the installation, as well as notes, details of the installation and location should be carefully checked.

4. Moldy waterproof tarpaulin will destroy the tent waterproof. So when the situation happens, You should use a sponge cleaner to remove mildew and then dried it.

5,The waterproof tarpaulin need to be of exposure in the sun after used for some time, which can prevent the emergence of bacteria. It is best to hang up the tent to dry.]

**4.What can we do to help prolong the life of our tarpaulins for truck cover?**Now, in our lives, tarpaulin for truck cover is very common. It can be rain-proof and sun resistant so that to protect truck. So when we use it, what should we notice? And what can we do to help prolong the life of our tarpaulins for truck cover. Please see the following.
We should notice the followings when we use tarpaulin for truck cover.
1.First , we should ensure that the tarp in both sides of the vehicle that the height are the same, the car number are exposed.
2. Note that tarpaulin is only applicable to open car. One tarpaulin for one car.
3.Tarpaulin is flat, no cargo exposed. From the top of the ridge, both sides of the package angle are closed; smooth lines are on both sides. The size of each part does not exceed the limit.
4.The length of tarpaulin for the end cover of truck hand brake is no more than 500mm. If the hand brake disc of truck is exposed, it will not affect the use of hand brake disc and mention hook rod.
5.Tie a solid knot to rope and tie it to the right position, no relaxation off. The knot of rope tied to the T-shaped iron looks like a butterfly’s wing. The tail length of rope is from 100mm to 300mm.

**5. How to effectively remove the smell of tarpaulin products**

When we use the tarpaulin products, we should also have encountered such a situation. Due to the wrong location or the wet tarpaulin, the product will be moldy. At this time, there will appear the terriable smell of tarpaulin products. So, what methods can be used to effectively remove the smell of the product?

If we want to remove the smell, we should first find out the reasons. Generally, the mold grows up in a relatively humid place and will be of mass reproduction in a humid environment. So we do not put it in a wet environment. Secondly, we can also use soapy water, sponge to wipe the tarpaulin. Sponge glue on the hot water, cleaning agent can wipe the tent clean. As well as the use of salt, lemon juice, gallons of water mixing, then knead to poke in dry mildew can also remove odor, mildew.